|  |
| --- |
| G:\6100_Performance_HR\6555 - Organisational Safety and Wellbeing\2. HSW - Systems and Strategy Team\Rebadging OSW Documents (Kristyn)\ITD logos\Updated 2018\Welding_word_banner_SOP.jpg  **MMA WELDER** |
|  |
| **DO NOT** use this equipment unless a teacher has instructed you in its safe use and operation and has given permission |

|  |  |
| --- | --- |
| Approved safety glasses must be worn at all times in addition to a welding helmet. | Hair Protection circleLong and loose hair must be contained or restrained. |
| Foot Protection circleAppropriate protective footwear with substantial uppers must be worn. | ApronClose fitting protective clothing or overalls, leather apron and spats must be worn. |
| Appropriate welding mask with correct grade lensWelding Mask circle must be worn | Hand Protection circleOil free leather gloves must be worn when using this equipment. |
| Prohibition circleRings and jewellery must not be worn. | Pacemaker caution sign02 |
|  |  |

### **PRE-OPERATIONAL SAFETY CHECKS**

1. **Check workspace to ensure that no slip/trip hazards are present.**
2. **Check work area is clean and free of grease, oil and flammable material.**
3. **Ensure the equipment and work area is dry to avoid electric shocks.**
4. **Inspect gloves to ensure they are free from holes and are dry to avoid electric shocks.**
5. **Check the electrode holder and work leads are in good condition.**
6. **Ensure the fume extractor unit is on before welding commences.**
7. **Close the UV curtain or erect safety screens to ensure the protection of others.**

**DO NOT** use faulty equipment – report this immediately to your teacher.

OPERATIONAL SAFETY CHECKS

1. **Keep the welding leads as short as possible and coil them to minimise inductance.**
2. **Ensure the electrode holder has no electrode in it before turning on the welder.**
3. **Ensure current is correctly set according to electrode selection.**
4. **Do not use bare hands and never wrap electrode leads around yourself.**
5. **When welding is finished or interrupted, remove electrode stub from holder and switch off power source.**

HOUSEKEEPING

1. **Switch off the machine and fume extraction.**
2. **Hang up electrode holder and welding cables and leave the work area in a safe, clean and tidy state.**

#### POTENTIAL HAZARDS

* **Electric shock ◼ Radiation burns to eyes or body ◼ Flying sparks ◼ Fire**
* **Fumes ◼ Body burns due to hot or molten materials ◼ Cuts and lacerations**

