|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Regular servicing as per maintenance checklist/major or minor repairs** | **Maintenance performed by company/business/individual** | **Time taken** | **Cost**  | **Tag-out (if required)** | **Tag removed and checked by** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

## **Maintenance record – equipment/machinery**

|  |
| --- |
| **The below checks are recommended for equipment prior to or during a unit of work where the equipment will undergo moderate to heavy use.** |
| Equipment/machine checks  | **Date** |  / / |  / / |  / / |  / / | **Follow-up actions** |
| **Signature** |  |  |  |  |
|  | Tick or comment✓ | Tick or comment✓ | Tick or comment✓ | Tick or comment✓ | E.g. cracked blade replaced 03/18John Smith |
| Check the **press frame** for damage and that all nuts and bolts are tight and secure. |  |  |  |  |  |
| Ensure **V blocks** and any other accessories are in good condition. |  |  |  |  |  |
| **Lubricate** lightly according to manufacturer’s specification (pivot points and moving parts etc.) |  |  |  |  |  |
| Ensure pressure **gauge** and release **valve** (where fitted) is functioning correctly. |  |  |  |  |  |
| Ensure **winch** mechanism is operating effectively (where fitted).  |  |  |  |  |  |
| Check support pins and height location holes are in good condition – free from damage. |  |  |  |  |  |
| Ensure hydraulic press is **secured** firmly to floor. |  |  |  |  |  |
| Other: |  |  |  |  |  |
| Other: |  |  |  |  |  |
| Other: |  |  |  |  |  |
| Other:  |  |  |  |  |  |
| Other:  |  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **End of semester checks**  | **Date**  |  / / |  / / | **Follow-up actions** |
| **Signature** |  |  |
| **Tick or comment****✓**  | **Tick or comment****✓**  | E.g. blade and pulley alignment adjusted 02/18John Smith |
| **Sem 1**  | **Sem 2** |
| **Lubricate** all points in accordance with the manufacturer's specification. |  |  |  |
| **Protect** all **bare metal** surfaces before term shutdown (CRC, WD40, RP7 of similar). |  |  |  |
| Check the **press frame** for damage and that all nuts and bolts are tight and secure. |  |  |  |
| Ensure **V blocks** and any other accessories are in good condition. |  |  |  |
| **Lubricate** lightly according to manufacturer’s specification (pivot points & moving parts etc.) |  |  |  |
| Ensure pressure **gauge** and release **valve** (where fitted) is functioning correctly. |  |  |  |
| Ensure **winch** mechanism is operating effectively (where fitted).  |  |  |  |
| Check support pins and height location holes are in good condition – free from damage. |  |  |  |
| Ensure hydraulic press is **secured** firmly to floor. |  |  |  |
| Other:  |  |  |  |
| Other:  |  |  |  |
| Other:  |  |  |  |

|  |  |
| --- | --- |
| **Annual check *Date*** ***Signature*** |  / / |
|  |
| **Tick or comment****✓** |
| Check condition of **50mm line markings** defining operator zones and access walkways. |  |
| **Review safety operating procedure** and **update** if necessary. |  |
| **Other:** |  |
| **Other:** |  |
| **Other:** |  |
| **Other:** |  |
| **Other:** |  |
| **Follow-up actions** e.g. Yellow line for operator zone repainted14/12 John Smith |
|  |
|  |
|  |
|  |
|  |
|  |
|  |