
Using the Department’s removable asbestos label suitable supplier list
Introduction
Section 13.6 of the Working on Department of Education facilities document requires service providers conducting project work[footnoteRef:1] on Department of Education (DoE) facilities to: [1:  Works aimed at achieving a specific built improvement to departmental facilities through a planned approach. Projects may be of a ‘minor’ or ‘capital’ nature.
] 

· before commencing the works:
· identify, in writing, the presence of assumed or confirmed asbestos containing materials (ACM) in the work and adjoining areas;
· affix removable asbestos labels, that are compliant with DoE requirements, to assumed and confirmed ACM surfaces in the areas;
· ensure the labels remain for the duration of the project works and are removed at the conclusion of the works.
Refer section 13.6 for the full requirements, including label placement. 
A market sounding request process was conducted by DoE to establish a list of suitable label suppliers with products that could meet departmental removable asbestos label requirements. This list has been published to enable building and construction service providers, conducting work on DoE facilities, timely identification of suitable suppliers. The publishing of the list does not prohibit service providers from sourcing compliant labels from other label suppliers. The list will be updated periodically. 
Project work service provider steps for using this list
1. Select desired supplier and associated label product from the below Removable asbestos label suitable supplier list
2. Prepare the label artwork: 
a. Download the Department-approved asbestos label artwork and save to file in in pdf format;
b. If a JPEG file format is required for the print designer, screenshot the label artwork and save as a JPEG;
3. Follow the ordering instructions for the selected supplier.
Tips
· Ensure sufficient time is allowed for production and shipping of labels to prevent project delays.
· Labels may be suitable for re-use if suitable markers are used for recording ACM ID numbers.
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Removable asbestos label suitable supplier list	Last updated: 6 July 2026
	Business name
	AAC Wristbands Australia Pty Ltd
	Avery
	Biz Labels

	Web address
	https://aac.com.au
	https://www.averyproducts.com.au
	https://www.bizlabels.com.au

	Suitable product options
	Vinyl stickers
Fabric stickers
	Custom Printed Removable Heavy Duty Waterproof Labels and Stickers
	White gloss removable vinyl
Fabric wall decals

	Ordering method
	Online – Vinyl stickers
Email – Fabric stickers
	Online store
	Online store or
Email order

	Customer support
	sales@aac.com.au
(07) 5665 9333
	info@avery.com.au 
1800 644 353
	info@bizlabels.com.au
(07) 3175 3755

	Nominated timeframe from order to dispatch
	5-7 business days following artwork approval
Faster turnaround available if requested
	1-2 business days
	1-7 days
Dependent on size and quantity of labels

	Order streamlining opportunities
	Customer account creation holds contact info, artwork files, specifications, addresses etc for repeat orders
	Quick re-order and fast checkout for account holders
	-

	In-store pick-up option
	Yes
	No
	Yes

	In-store immediate print option
	No
	
No
	No




Ordering instructions
AAC Wristbands
Vinyl stickers
1. Navigate to the AAC webpage (link in table above)
2. Select from the product menu – Stickers, then Square vinyl stickers
3. In size drop down menu, select 150mm (closes size to minimum size specified by DoE requirements)
4. In material drop down menu, select White vinyl
5. In decoration drop down menu, select Printed 
6. Enter quantity required
7. Click Design & Add to cart 
8. The online designer will open  on the left side menu, click Images  Upload
9. Select JPEG file of the label artwork and upload unto designer (click or drag and drop where prompted)
10. Scale and position artwork as required
11. Click Add to cart  Checkout now
12. Enter shipping information and click Proceed to checkout
Fabric stickers
Email order request (address in table above) including the following details:
· Size requirement (minimum 135 x 95mm)
· Specify ‘Fabric stickers’
· Provide artwork (e.g. attach downloaded pdf or jpeg file to the email)
· Quantity required
· Shipping details 
Avery Products
1. Navigate to the Avery Products webpage (link in table above)
2. Search or find in the products menu – Removable Heavy Duty Waterproof (or use direct link in table above)
3. Select the rectangle shape option
4. Choose the 135 x 95mm size option
5. Select Removable Heavy Duty material option
6. Select quantity of labels required 
7. Click Start designing  In the pop-up window, click Upload your artwork
8. Upload asbestos label artwork pdf file
9. Scale and position artwork as required using the online designer tool  Click finish 
10. Process order in online store including payment and shipping details

BizLabels
Online store
1. Navigate to the BizLabels website (link in table above)
2. Create an account or login using account details
3. Select from the product menu – 
a. Bumper stickers – select material: White gloss removable vinyl; or
b. Fabric wall decals
4. Input label size in provided boxes (135 x 95mm)
5. Select quantity of labels required
6. Click Design your own
7. Click Uploads and select asbestos label artwork (jpeg file format required)
8. Scale and position artwork as required using the online designer tool  Click Continue
9. Review order details and click Add to cart
10. Add additional products as required. From the cart, click Proceed to checkout
11. Process order in online store including payment and shipping details

Email order
Email order request (address in table above) including the following details:
· Size requirement (minimum 135 x 95mm)
· Specify ‘Fabric wall decals’ or ‘Removable vinyl stickers’
· Provide artwork (e.g. attach downloaded pdf or jpeg file to the email)
· Quantity required
· Shipping details 

Service provider feedback
Contact Infrastructure.Safety@qed.qld.gov.au if you are a service provider:
· experiencing issues applying the ordering instructions; or
· who has concerns regarding the quality of labels sourced using the instructions.

Supplier enquiries
Contact Infrastructure.Safety@qed.qld.gov.au if you are a business:
· on the suitable supplier list and would like changes to your published details; or
· who would like to be assessed under the market sounding request process for inclusion on the suitable supplier list.
Note: suppliers will be removed from the list if they are unable to demonstrate specification compliance during departmental assurance activities or following the department receiving information to indicate non-compliance.

image1.jpg
Queensland Government

SELIVERING | S Queensland

FOR QUEENSLAND J' Government





