|  |
| --- |
| ***Portable_Plant_SOP*****NAIL GUN (cordless)**🗹 |
| ***Students must complete the checklist below with a tick in every box before operating this portable power equipment*** |
| **Has your teacher given you instruction on the safe use and operation of this equipment?** | **🗆** |
|  |
| **Has your teacher given permission for you to use this equipment?** | **🗆** |
|  | Are you wearing approved safety glasses and face shield?. | **🗆** |
| Foot Protection circle | Are you wearing protective steel-toed work boots?. | **🗆** |
| Hearing Protection circle | Do you, and others around you, have appropriate hearing protection? *(Class 5 – SLC80 >26 dB)* | **🗆** |
| Hard hat | Are you wearing a hard hat on worksites hen required?  | **🗆** |
| mand154_safety_overalls_must_ | Are you wearing workwear clothing or overalls?  | **🗆** |
| Prohibition circle | Have you removed all your exposed rings and jewellery?  | **🗆** |
| **Have you read the important information section on the reverse?** | **🗆** |
|  **PRE-OPERATIONAL SAFETY CHECKS** |  |
| 1. Has the actuation muzzle been serviced and checked for safe operation?
 | **🗆** |
| 1. Has an exclusion zone been established with barricading and appropriate safety signage?
 | **🗆** |
| 1. Are you aware of departmental safety alerts for the equipment? (check with your teacher)
 | **🗆** |
| 1. Are you familiar with the type of nail gun you are about to operate and how it is powered? i.e. battery or explosive gas
 | **🗆** |
| 1. If a pneumatic nail gun is to be used, has the air compressor been inspected and checked for safe operation use?
 | **🗆** |
| 1. Have you inspected the equipment for any obvious mechanical defects?
 | **🗆** |

Paste pages 1 and 2 back to back – cut out this section – laminate and trim to size

Nail Gun (cordless)

|  |
| --- |
| ***Portable_Plant_SOP*****NAIL GUN (cordless)****Air Compressor** |
| **Important information – read before use** |
| **OPERATIONAL SAFETY CHECKS** |
| **DO NOT use faulty equipment – report this immediately to your teacher** |
| 1. Never attempt to operate this power tool if you are an inexperienced worker without proper training.
2. The nail gun user and everyone working within the vicinity should be wearing safety glasses. Protective footwear and hearing protection should also be worn.
3. Be very aware of others who may be working nearby.
4. Keep your finger off the trigger when not firing nails. The centre of gravity at the trigger makes it easy to accidentally fire the nail gun.
5. NEVER use a nail gun with a missing push lever and muzzle safety sprint (or safety yoke).
6. Always keep your hands and feet away from the muzzle of the nail gun.
7. Never use any part of your body to support the material you are nailing.
8. Never rest the nail gun against any body part, or try to climb a ladder with the nail gun cradled against your body. Never point a nail gun at anyone.
9. Always disconnect the nail gun from its power source before transporting, reloading or trying to free a jammed nail.
10. Never leave any nail gun unattended.
 |
|  |
| **NEVER use a bump-fire nail gun in a school workshop environment** |
|  |
| **HOUSEKEEPING** |
| 1. Leave the power tool and work area in a safe, clean and tidy state.
2. Maintain correct operation of the actuation mechanism. Store away safely.
 |
|  |
| **POTENTIAL HAZARDS** |
| ◼ Moving, sharp parts ◼ Flammable gases ◼ Pinch and squash ◼ Ejected material ◼ Excessive noise ◼ Eye injuries ◼ Slips, trips and falls ◼ Dust  |
|  |
| **FORBIDDEN** |
| * Students must never operate a nailing gun of any model or operational mode while working on ladders, high platforms or in confined spaces.
 |

 **Date of last review:**  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Signature:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_